How to Update the Firmware

Update the PROM code:

Modify the configure file for PROM code updating

Specify the directory path and image file name for PROM code.

Enable your TFTP server.

Enter console program; select Update Firmware and Configuration Files in the main menu.

Set the Software Update Mode to “Network”.

Specify the IP address of your TFTP server.

In the Configuration File field, Set Use Config Files to “Enable”

In File Name field, specify the path and file name of config file. The following screen appears:

Press RESET SWITCH TO START UPDATE to initiate the update sequence.

Restart the switch. Check the version of PROM code. is it the correct version you want to update?

Update the Runtime code:

Modify the configure file for RunTime code updating

Specify the directory path and image file name for RunTime code.

Enable your TFTP server.

Enter console program; select Update Firmware and Configuration Files in the main menu.

Set the Software Update Mode to “Network”.

Specify the IP address of your TFTP server.

In the Configuration File field, Set Use Config Files to “Enable”

In File Name field, specify the path and file name of config file. The following screen appears:

Press RESET SWITCH TO START UPDATE to initiate the update sequence.

Restart the switch. Check the version of PROM code. is it the correct version you want to update?

Written by: Simon Hsu

Dept. Technical Support

Updated: June 26, 2000

Code_type=PROM

Image_file="d:\des3624\3624prom.207"

#Code_type=RUNTIME

#Image_file="d:\switch\des3624\3624run.230"

#Code_type=CONFIG

#Image_file="g:\d-link\des-32~1\basic_25.bc"

# specify IP address

#Ip_addr = 10.9.68.25

# specify subnet mask

#Subnet_mask = 255.0.0.0

# specify default gateway

#Default_gateway = 10.254.254.254

#Code_type=PROM

#Image_file="d:\des3624\3624prom.207"

Code_type=RUNTIME

Image_file="d:\des3624\3624run.230"

#Code_type=CONFIG

#Image_file="g:\d-link\des-32~1\basic_25.bc"

# specify IP address

#Ip_addr = 10.9.68.25

# specify subnet mask

#Subnet_mask = 255.0.0.0

# specify default gateway

#Default_gateway = 10.254.254.254

How to Update the Firmware

Simon Hsu

2000-11-27

Donnie Viajar

D-Link